# Pulsadores

NET "clk" LOC = "B8";

NET "reset" LOC = "A7";

#NET "wr" LOC = "M4";

# rx & tx

NET "rx" LOC = "B5";

NET "tx" LOC = "J3";

# Flags full empty

NET "rx\_empty" LOC = "L14"; //M5

NET "tx\_full" LOC = "N11"; //P4

# LED

NET "result\_alu<0>" LOC = "M5";

NET "result\_alu<1>" LOC = "M11";

NET "result\_alu<2>" LOC = "P7";

NET "result\_alu<3>" LOC = "P6";

NET "result\_alu<4>" LOC = "N5";

NET "result\_alu<5>" LOC = "N4";

NET "result\_alu<6>" LOC = "P4";

NET "result\_alu<7>" LOC = "G1";